# FluoviewReader

This page lists supported metadata fields for the Bio-Formats Olympus Fluoview/ABD TIFF format reader.

These fields are from the OME data model. Bio-Formats standardizes each format’s original metadata to and from the OME data model so that you can work with a particular piece of metadata (e.g. physical width of the image in microns) in a format-independent way.

Of the 476 fields documented in the metadata summary table:

  - The file format itself supports 49 of them (10%).

  - Of those, Bio-Formats fully or partially converts 49 (100%).

## Supported fields

These fields are fully supported by the Bio-Formats Olympus Fluoview/ABD TIFF format reader:

  - Channel : ID

  - Channel : Name

  - Channel : SamplesPerPixel

  - Detector : ID

  - Detector : Manufacturer

  - Detector : Model

  - Detector : Type

  - DetectorSettings : Gain

  - DetectorSettings : ID

  - DetectorSettings : Offset

  - DetectorSettings : ReadOutRate

  - DetectorSettings : Voltage

  - Image : AcquisitionDate

  - Image : Description

  - Image : ID

  - Image : InstrumentRef

  - Image : Name

  - ImagingEnvironment : Temperature

  - Instrument : ID

  - Objective : CalibratedMagnification

  - Objective : Correction

  - Objective : ID

  - Objective : Immersion

  - Objective : LensNA

  - Objective : Model

  - ObjectiveSettings : ID

  - Pixels : BigEndian

  - Pixels : DimensionOrder

  - Pixels : ID

  - Pixels : Interleaved

  - Pixels : PhysicalSizeX

  - Pixels : PhysicalSizeY

  - Pixels : PhysicalSizeZ

  - Pixels : SignificantBits

  - Pixels : SizeC

  - Pixels : SizeT

  - Pixels : SizeX

  - Pixels : SizeY

  - Pixels : SizeZ

  - Pixels : TimeIncrement

  - Pixels : Type

  - Plane : DeltaT

  - Plane : ExposureTime

  - Plane : PositionX

  - Plane : PositionY

  - Plane : PositionZ

  - Plane : TheC

  - Plane : TheT

  - Plane : TheZ

Total supported: 49

Total unknown or missing: 427